Firmware upgrade using FlashMe v3.7

All copyrights reserved. Author: Klemen Pavlic (2010 - 2021).

THE SOFTWARE IS PROVIDED "AS IS" AND THE AUTHOR DISCLAIMS ALL WARRANTIES WITH REGARD TO THIS SOFTWARE INCLUDING ALL IMPLIED WARRANTIES OF MERCHANTABILITY AND FITNESS. IN NO EVENT SHALL THE AUTHOR BE LIABLE FOR ANY SPECIAL, DIRECT, INDIRECT, OR CONSEQUENTIAL DAMAGES OR ANY DAMAGES WHATSOEVER RESULTING FROM LOSS OF USE, DATA OR PROFITS, WHETHER IN AN ACTION OF CONTRACT, NEGLIGENCE OR OTHER TORTIOUS ACTION, ARISING OUT OF OR IN CONNECTION WITH THE USE OR PERFORMANCE OF THIS SOFTWARE.

Permission to use is granted only to customers of our measuring instruments.


INSTRUCTIONS FOR AUTOMATIC UPGRADE:

1.) Press power on/off key to turn on the instrument.

2.) Connect the instrument to a PC using a serial or an USB(*1*) cable.

3.) Extract the attached zip file.

4.) Double click on the "upgrade-automatic.vbs" file. This should start the FlashMe application.

5.) Select the com port, to which the instrument is connected to. If you're using an USB connection look for a com port, which in it's description contains the words "MeasuringInstrumentUsb".

6.) Click the RUN button and afterward click the CONTINUE button.

7.) Wait until FlashMe signals the end of firmware upgrade.


INSTRUCTIONS FOR MANUAL UPGRADE:

1.) Press POWER ON/OFF key while simultaneously holding down the ENTER key, until the FlashMe logo appears on the instruments screen.

2.) Connect the instrument to a PC using a serial or an USB(*1*) cable.

3.) Extract the attached zip file.

4.) Double click on the "upgrade-manual.vbs" file. This should start the FlashMe application.

5.) Select the com port, to which the instrument is connected to. If you're using an USB connection look for a com port, which in it's description contains the words "MeasuringInstrumentUsb".

6.) Click the RUN button and afterward click the CONTINUE button.

7.) Wait until FlashMe signals the end of firmware upgrade.

(*1*) When using an USB connection for the first time, operating system will inform you, that it needs to install the USB driver. Cancel the automatic installation and manually point the installer the folder to which the zip file was extracted to. This folder must contain the file "vcom.inf".
You can also do this manually. Open the device manager, find the device (MeasuringInstrumentUsb), right click and select "Upgrade  driver software". Point to the folder containing the file "vcom.inf".